{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["PHD Attribute Locations","Form&Doc PWise Location"],"not_rendered":{"images":1,"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"PHD Attribute Locations","index":0,"n_rows":221,"n_cols":5,"rows_kept":221,"merged":[[0,0,0,1],[0,2,0,4],[2,0,9,0],[10,0,12,0],[15,0,19,0],[20,0,21,0],[22,0,24,0],[25,0,27,0],[28,0,31,0],[32,0,39,0],[40,0,46,0],[51,0,52,0],[54,0,58,0],[62,0,73,0],[74,0,80,0],[81,0,92,0],[93,0,104,0],[105,0,117,0],[118,0,130,0],[131,0,143,0],[144,0,155,0],[156,0,162,0],[164,0,169,0],[172,0,176,0],[177,0,186,0],[187,0,203,0],[205,0,206,0],[207,0,211,0],[212,0,214,0],[215,0,218,0]]}
["PHD Data Items",null,"Form Number / Document (last updated 11/01/2023)"]
["Layer","Attribute","1st Choice","2nd Choice","3rd Choice"]
["Agg. Base Course – Cement Stab.","Cement content","Ticket","MSL/0501"]
[null,"Fly ash content ","Ticket","MSL/0501"]
[null,"GGBFS","Ticket","MSL/0501"]
[null,"Portland Cement supplier","MSL/0501"]
[null,"Portland Cement type","MSL/0501","Ticket"]
[null,"Thickness","IDR/1122B","Plans/Proposal"]
[null,"Aggregate class",1900,"MSL/0501"]
[null,"Source (pit number)",1900,"MSL/0501"]
["Aggregate Base Course","Thickness","IDR/1122B","Plans/Proposal"]
[null,"Aggregate class",1900,"MSL/0501"]
[null,"Source (pit number)",1900,"MSL/0501"]
["Brick Pavers","Thickness","IDR/1122B","Plans/Proposal"]
["Brick Seal","Brick Seal (yes/no)","IDR/1122B","Plans/Proposal"]
["Chip Seal","Emulsion","MSL/0501","12SP-505A-04"]
[null,"Emulsified asphalt supplier","MSL/0501"]
[null,"Number of courses","IDR/1122B","Plans/Proposal"]
[null,"Aggregate class",1900,"MSL/0501"]
[null,"Source (pit number)",1900,"MSL/0501"]
["Cold In Place Recycled Asphalt","Emulsion","MSL/0501","Special Provision"]
[null,"Thickness","IDR/1122B","Plans/Proposal"]
["Cold Milling","Cold Milling Depth","IDR/1122B","Plans/Proposal"]
[null,"Cold Milling Texture","IDR/1122B","Plans/Proposal"]
[null,"Cold Milling Type","IDR/1122B","Plans/Proposal"]
["Concrete Pavement Crack/Joint Sealing","Crack sealing (yes/no)","IDR/1122B","MSL/0501","Plans/Proposal"]
[null,"Resealing longitudinal joints (yes/no)","IDR/1122B","Plans/Proposal"]
[null,"Resealing transverse joints (yes/no)","IDR/1122B","Plans/Proposal"]
["Concrete Pavement Repairs (Detail 7’s & 8’s)","Detail 7’s placed (yes/no)","IDR/1122B","Plans/Proposal"]
[null,"Detail 7 mix type",1911,"1903B","Plans/Proposal"]
[null,"Detail 8’s placed (yes/no)","IDR/1122B","Plans/Proposal"]
[null,"Detail 8 mix type",1911,"1903B","Plans/Proposal"]
["Concrete Pavement Repairs (Full Depth)","Cement content",1976]
[null,"Concrete Grade","1174R"]
[null,"Portland Cement supplier",1976,1155,"MSL/0501"]
[null,"Portland Cement type",1976,1155,"MSL/0501"]
[null,"Reinforcement steel (yes/no)","IDR/1122B","MSL/0501","Plans/Proposal"]
[null,"Thickness","IDR/1122B","Plans/Proposal"]
[null,"Aggregate class",1976,1155,"MSL/0501"]
[null,"Source (pit number)",1976,1155,"MSL/0501"]
["Concrete Pavement Repairs (Partial Depth)","Cementitious Repair? (yes/no)","IDR/1122B","MSL/0501","Plans/Proposal"]
[null,"Prepackaged Mortar Product","Material Cert/Cert of Compliance/Cert of Analysis","MSL/0501"]
[null,"Cement supplier",1976,1155,"MSL/0501"]
[null,"Cement type",1976,1155,"MSL/0501"]
[null,"Non-cementitious Product","Material Cert/Cert of Compliance/Cert of Analysis","MSL/0501"]
[null,"Aggregate class",1976,1155,"MSL/0501"]
[null,"Source (pit number)",1976,1155,"MSL/0501"]
["Concrete Penetrating Sealer","Silane Material","Material Cert/Cert of Compliance/Cert of Analysis","IDR/1122B","MSL/0501"]
["Crack Relief Interlayer/DRM","Thickness","IDR/1122B","Plans/Proposal"]
["Cracked and Seated Concrete","Thickness","IDR/1122B","Plans/Proposal"]
["Crushed and Shaped HMA","Thickness","IDR/1122B","Plans/Proposal"]
["Diamond Grinding/Grooving","Diamond Grinding (yes/no)","IDR/1122B","Plans/Proposal"]
[null,"Longitudinal Grooving (yes/no)","IDR/1122B","Plans/Proposal"]
["Dowel Bar Retrofit","Dowel Bar Retrofit (yes/no)","IDR/1122B","Plans/Proposal"]
["FiberMat","Emulsion","Material Cert/Cert of Compliance/Cert of Analysis","MSL/0501"]
[null,"Emulsified Asphalt Supplier","Material Cert/Cert of Compliance/Cert of Analysis","MSL/0501"]
[null,"FiberMat type","IDR/1122B","MSL/0501","Plans/Proposal"]
[null,"Aggregate class",1900,"MSL/0501"]
[null,"Source (pit number)",1900,"MSL/0501"]
["Fog Seal","Fog Seal (yes/no)","IDR/1122B","MSL/0501","Plans/Proposal"]
["Geotextile Fabric","Geotextile type","IDR/1122B","Plans/Proposal","MSL/0501"]
["High Friction Surface","High Friction Surface placed (yes/no)","IDR/1122B","Plans/Proposal"]
["HMA Base Course","Mix type",1911,"1903B","Plans/Proposal"]
[null,"Mix design number (case sensitive)",1911,"1903B"]
[null,"Application rate","Yield Calculations","Plans/Proposal"]
[null,"Asphalt binder",1911,"1903B","MSL/0501"]
[null,"Asphalt binder certified supplier",1911,"1903B","MSL/0501"]
[null,"Asphalt % (Total)",1911]
[null,"Asphalt Binder %Added (Virgin)",1911]
[null,"Warm Mix (yes/no)",1911,"IDR/1122B","Recorded HMA Temperatures"]
[null,"If Warm Mix, Water Foaming? (yes/no)",1911,"IDR/1122B"]
[null,"If Warm Mix, select the Additive",1911,"IDR/1122B","MSL/0501"]
[null,"Aggregate class",1911,"MSL/0501"]
[null,"Source (pit number)",1911,"MSL/0501"]
["HMA Crack Treatment","Cut and seal method","On Site Verification"]
[null,"HMA Crack Seal Manufacturer","Special Provision (12SP-914B-01)","Material Cert/Cert of Compliance/Cert of Analysis","MSL/0501"]
[null,"HMA Crack Seal Product","Special Provision (12SP-914B-01)","Material Cert/Cert of Compliance/Cert of Analysis","MSL/0501"]
[null,"Lab #",1922]
[null,"Lot #",1922]
[null,"Was Overband also used? – Yes/No","IDR/1122B","MSL/0501"]
[null,"Overband Crack Fill Product","Material Cert/Cert of Compliance/Cert of Analysis","MSL/0501"]
["HMA Leveling Course","Mix type",1911,"1903B","Plans/Proposal"]
[null,"Mix design number (case sensitive)",1911,"1903B"]
[null,"Application rate","Yield Calculations","Plans/Proposal"]
[null,"Asphalt binder",1911,"1903B","MSL/0501"]
[null,"Asphalt binder certified supplier",1911,"1903B","MSL/0501"]
[null,"Asphalt % (Total)",1911]
[null,"Asphalt Binder %Added (Virgin)",1911]
[null,"Warm Mix (yes/no)",1911,"IDR/1122B","Recorded HMA Temperatures"]
[null,"If Warm Mix, Water Foaming? (yes/no)",1911,"IDR/1122B"]
[null,"If Warm Mix, select the Additive",1911,"IDR/1122B","MSL/0501"]
[null,"Aggregate class",1911,"MSL/0501"]
[null,"Source (pit number)",1911,"MSL/0501"]
["HMA Separator Course","Mix type",1911,"1903B","Plans/Proposal"]
[null,"Mix design number (case sensitive)",1911,"1903B"]
[null,"Application rate","Yield Calculations","Plans/Proposal"]
[null,"Asphalt binder",1911,"1903B","MSL/0501"]
[null,"Asphalt binder certified supplier",1911,"1903B","MSL/0501"]
[null,"Asphalt % (Total)",1911]
[null,"Asphalt Binder %Added (Virgin)",1911]
[null,"Warm Mix (yes/no)",1911,"IDR/1122B","Recorded HMA Temperatures"]
[null,"If Warm Mix, Water Foaming? (yes/no)",1911,"IDR/1122B"]
[null,"If Warm Mix, select the Additive",1911,"IDR/1122B","MSL/0501"]
[null,"Aggregate class",1911,"MSL/0501"]
[null,"Source (pit number)",1911,"MSL/0501"]
["HMA Skip Patching","Mix type",1911,"1903B","Plans/Proposal"]
[null,"Mix design number (case sensitive)",1911,"1903B"]
[null,"Application rate","Yield Calculations","Plans/Proposal"]
[null,"Asphalt binder",1911,"1903B","MSL/0501"]
[null,"Asphalt binder certified supplier",1911,"1903B","MSL/0501"]
[null,"Asphalt % (Total)",1911]
[null,"Asphalt Binder %Added (Virgin)",1911]
[null,"AWI (Actual)",1911]
[null,"Warm Mix (yes/no)",1911,"IDR/1122B","Recorded HMA Temperatures"]
[null,"If Warm Mix, Water Foaming? (yes/no)",1911,"IDR/1122B"]
[null,"If Warm Mix, select the Additive",1911,"IDR/1122B","MSL/0501"]
[null,"Aggregate class",1911,"MSL/0501"]
[null,"Source (pit number)",1911,"MSL/0501"]
["HMA Top Course","Mix type",1911,"1903B","Plans/Proposal"]
[null,"Mix design number (case sensitive)",1911,"1903B"]
[null,"Application rate","Yield Calculations","Plans/Proposal"]
[null,"Asphalt binder",1911,"1903B","MSL/0501"]
[null,"Asphalt binder certified supplier",1911,"1903B","MSL/0501"]
[null,"Asphalt % (Total)",1911]
[null,"Asphalt Binder %Added (Virgin)",1911]
[null,"AWI (Actual)",1911]
[null,"Warm Mix (yes/no)",1911,"IDR/1122B","Recorded HMA Temperatures"]
[null,"If Warm Mix, Water Foaming? (yes/no)",1911,"IDR/1122B"]
[null,"If Warm Mix, select the Additive",1911,"IDR/1122B","MSL/0501"]
[null,"Aggregate class",1911,"MSL/0501"]
[null,"Source (pit number)",1911,"MSL/0501"]
["HMA Ultra-Thin Overlay","Mix type",1911,"1903B","Plans/Proposal"]
[null,"Mix design number (case sensitive)",1911,"1903B"]
[null,"Application rate","Yield Calculations","Plans/Proposal"]
[null,"Asphalt binder",1911,"1903B","MSL/0501"]
[null,"Asphalt binder certified supplier",1911,"1903B","MSL/0501"]
[null,"Asphalt % (Total)",1911]
[null,"Asphalt Binder %Added (Virgin)",1911]
[null,"AWI (Actual)",1911]
[null,"Warm Mix (yes/no)",1911,"IDR/1122B","Recorded HMA Temperatures"]
[null,"If Warm Mix, Water Foaming? (yes/no)",1911,"IDR/1122B"]
[null,"If Warm Mix, select the Additive",1911,"IDR/1122B","MSL/0501"]
[null,"Aggregate class",1911,"MSL/0501"]
[null,"Source (pit number)",1911,"MSL/0501"]
["HMA Wedge Course","Mix type",1911,"1903B","Plans/Proposal"]
[null,"Mix design number (case sensitive)",1911,"1903B"]
[null,"Application rate","Yield Calculations","Plans/Proposal"]
[null,"Asphalt binder",1911,"1903B","MSL/0501"]
[null,"Asphalt binder certified supplier",1911,"1903B","MSL/0501"]
[null,"Asphalt % (Total)",1911]
[null,"Asphalt Binder %Added (Virgin)",1911]
[null,"Warm Mix (yes/no)",1911,"IDR/1122B","Recorded HMA Temperatures"]
[null,"If Warm Mix, Water Foaming? (yes/no)",1911,"IDR/1122B"]
[null,"If Warm Mix, select the Additive",1911,"IDR/1122B","MSL/0501"]
[null,"Aggregate class",1911,"MSL/0501"]
[null,"Source (pit number)",1911,"MSL/0501"]
["Hot In Place Recycled Asphalt","AWI (Actual)",1911]
[null,"Asphalt binder",1911,"MSL/0501"]
[null,"Asphalt binder certified supplier",1911,"MSL/0501"]
[null,"Mix design number",1911]
[null,"Thickness","Yield Calculations","Plans/Proposal"]
[null,"Aggregate class",1911,"MSL/0501"]
[null,"Source (pit number)",1911,"MSL/0501"]
["Joint/Crack Repair Mastic","Asphalt Repair Mastic Product","MSL/0501"]
["Micro-surface","Emulsified asphalt supplier","Microsurface JMF","MSL/0501"]
[null,"Emulsion","Microsurface JMF","MSL/0501"]
[null,"Number of courses","IDR/1122B","Plans/Proposal"]
[null,"Rut Fill Layer","IDR/1122B","Plans/Proposal"]
[null,"Aggregate class","Microsurface JMF","MSL/0501"]
[null,"Source (pit number)","Microsurface JMF","MSL/0501"]
["Overband Crackfill","Overband Crack Fill Product","Material Cert/Cert of Compliance/Cert of Analysis","MSL/0501"]
["Pavement Jacking","Poly Pavement Jacking (yes/no)","IDR/1122B","Plans/Proposal"]
["Paver Placed Surface Seal","AWI (Actual)","MSL/0501"]
[null,"Application Rate","IDR/1122B","12SP-503A-02"]
[null,"Asphalt binder","12SP-503A-02","MSL/0501"]
[null,"Asphalt certified supplier","MSL/0501"]
[null,"PPSS mix type","IDR/1122B","Plans/Proposal"]
["PCC Pavement","Cement content",1976]
[null,"Fly ash content ",1976]
[null,"GGBFS",1976]
[null,"Portland Cement supplier",1976,1155,"MSL/0501"]
[null,"Portland Cement type",1976,1155,"MSL/0501"]
[null,"Thickness","IDR/1122B","Plans/Proposal"]
[null,"Transverse joint spacing","MDOT Std Plan R-43"]
[null,"Transverse joints sealed (yes/no)","IDR/1122B"]
[null,"Aggregate class",1976,1155,"MSL/0501"]
[null,"Source (pit number)",1976,1155,"MSL/0501"]
["Precast Concrete Pavement","Cement Content",1976]
[null,"Fly Ash Content",1976]
[null,"GGBFS",1976]
[null,"Portland Cement supplier",1976]
[null,"Portland Cement type",1976]
[null,"Post-Tensioned? (yes/no)","12DS603(E700)"]
[null,"Precast System","12DS603(E700)","Plans/Proposal"]
[null,"Pre-Stressed? (yes/no)","12DS603(E700)"]
[null,"Reinf Bar Steel, longitudinal","12DS603(E700)","Plans/Proposal"]
[null,"Reinf Bar Steel, transverse","12DS603(E700)","Plans/Proposal"]
[null,"Reinforcement Steel Mesh? (yes/no)","12DS603(E700)","Plans/Proposal"]
[null,"Repair (work <50’ & non-cont.)? (yes/no)","Plans/Proposal"]
[null,"Slab Length (typ joint spacing)","12DS603(E700)","Plans/Proposal"]
[null,"Thickness","Plans/Proposal","1174R"]
[null,"Transverse joints sealed (yes/no)","IDR/1122B"]
[null,"Aggregate class",1976,"MSL/0501"]
[null,"Source (pit number)",1976,"MSL/0501"]
["Roadway Embankment","Embankment placed below pavement? (yes/no)","IDR/1122B","Plans/Proposal"]
["Rubblized Concrete Pavement","Thickness","IDR/1122B","Plans/Proposal"]
[null,"Rubblizing Equipment Type","IDR/1122B","Plans/Proposal"]
["Scrub Seal","Number of courses","IDR/1122B","Plans/Proposal"]
[null,"Emulsified asphalt supplier","Material Cert/Cert of Compliance/Cert of Analysis","MSL/0501"]
[null,"Emulsion","Material Cert/Cert of Compliance/Cert of Analysis","MSL/0501","12DS505(M020)"]
[null,"Aggregate class",1900,"MSL/0501"]
[null,"Source (pit number)",1900,"MSL/0501"]
["Subbase","Thickness","IDR/1122B","Plans/Proposal"]
[null,"Aggregate class",1900,"MSL/0501"]
[null,"Source (pit number)",1900,"MSL/0501"]
["Subgrade Stabilization","Application Rate","IDR/1122B","Plans/Proposal"]
[null,"Stabilization Material","IDR/1122B","MSL/0501"]
[null,"Stabilization Material Type","IDR/1122B","MSL/0501"]
[null,"Thickness","IDR/1122B","Plans/Proposal"]
["Subgrade Undercut","Thickness","Form 0583","IDR/1122B","Plans/Proposal"]
["Void Reducing Asphalt Membrane","VRAM Application (per PR dir.) (Left/Right/Both)","Plans/Proposal","IDR/1122B","MSL/0501"]

{"sheet":"Form&Doc PWise Location","index":1,"n_rows":2,"n_cols":14,"rows_kept":2}
[]
[{"$nulls":13},"<--double click to open PDF"]