Steel erection continues to be a high hazard occupation. However, planning and forethought can provide employees with a safer work environment that will allow employers to maximize productivity and minimize costs due to lost time accidents. Falls are the number one cause of accidents and fatalities in the construction industry and are one of the most serious hazards that iron workers are exposed to.

Construction Standard [Part 26, Steel Erection](https://www.michigan.gov/leo/-/media/Project/Websites/leo/Documents/MIOSHA/Standards/Construction/CS_26/CS_26__04-03-2014.pdf?rev=dc682166afdd4fcf92a189081550d08c&hash=C6D99FC6215D20498F364AC41708B302) (Part 26) Rule 2645(1) requires fall protection for employees engaged in steel erection activity, when they are exposed to a fall of more than 15 feet above a lower level. Fall protection includes **guardrail systems, safety net systems, personal fall arrest systems, positioning device systems, or fall restraint systems**.

In addition to the fall protection systems above, there are alternate fall protection provisions in Part 26 that cover **connectors** and employees working in a **controlled decking zone**.

**Who is a connector?** A connector is an employee who, working with hoisting equipment, is placing and connecting structural members or components. In the Part 26 rulemaking process, it was intended that the definition be as narrow as possible, and the final definition of a connector carries out this intention. The definition is very specific; connection is distinguished from other steel erection activities by the elements of the definition. For example, spreading and securing bar joists by hand would not be considered connecting, since this work is not done with hoisting equipment. Therefore, an employee is a connector **only** when working with hoisting equipment. This includes placing components as they are received from hoisting equipment, and then connecting those components while hoisting equipment is overhead.

**What is hoisting equipment?** Hoisting equipment includes, but is not limited to, commercially manufactured cranes, derricks, tower cranes, barge mounted derricks or cranes, gin poles, gantry hoist systems, and fork trucks. The definition specifically excludes a “come along” as being considered hoisting equipment.

**Connector fall protection requirements:** Rule 2646 details the requirements and procedures for fall protection for connectors. When an employee is determined to be a connector in accordance with the definitions, the following provisions apply:

* At heights more than 30 feet, connectors must be provided and use fall protection. Fall protection includes guardrail systems, safety net systems, personal fall arrest systems, positioning device systems, or fall restraint systems.
* At heights more than 15 feet and up to 30 feet, connectors must wear fall protection equipment with the ability to be tied off, unless guardrail systems or safety net systems are in place. As soon as the worker is no longer connecting, they must utilize their fall protection equipment. The equipment worn would include full body harness, lanyard with appropriate deceleration device, and suitable anchorage equipment.
* Each employee working as a connector must have completed connector training in accordance with Part 26 Rule 2655(2).

**Employees working in a Controlled Decking Zone (CDZ):** While metal decking is being installed, the installers must be protected by the use of **guardrail systems, safety net systems, personal fall arrest systems, positioning device systems, or fall restraint systems** when they are exposed to a fall of more than 15 feet above a lower level. Installation of perimeter safety cables must be installed as soon as the metal deck is installed and prior to final deck attachments being completed. A CDZ may be established in an area of the structure of more than 15 feet and up to 30 feet above a lower level where the metal decking is being initially installed and forms a leading edge of a work area.

**What is a leading edge?** A leading edge is the unprotected side and edge of a floor, roof, or formwork for a floor, or other walking/working surface, such as a deck, which **changes location** as additional floor, roof, decking, or formwork sections are placed, formed or constructed.

**CDZ worker fall protection and other requirements:** Rule 2648 details the requirements and procedures to be followed for use of a CDZ. All the following provisions apply:

* A controlled decking zone may be established in that area of the structure of more than 15 and up to 30 feet above a lower level where metal decking is initially being installed and forms the leading edge of a work area. Each employee working at the leading edge in a CDZ shall be protected from fall hazards of more than 2 stories or 30 feet (9.1 m), whichever is less.
* Access to a CDZ shall be limited to those employees engaged in leading edge work.
* The boundaries of the CDZ shall be designated and clearly marked. The CDZ shall not be more than 90 feet wide and 90 feet deep from any leading edge. The CDZ shall be clearly marked by the use of control lines or the equivalent.
* Each employee working in a CDZ shall have completed CDZ training in accordance with Part 26, Rule 2655(3).
* Unsecured decking in a CDZ shall not be more than 3,000 square feet.
* Safety deck attachments shall be performed in the CDZ from the leading edge back to the control line and shall have not less than 2 attachments for each metal decking panel.
* Final deck attachments and installation of shear connectors shall not be performed in the CDZ.

**Other steel erection activities:** Each employee who is engaged in other steel erection work activities such as but not limited to decking, bolting, and welding, shall be protected from fall hazards at more than 15 feet by the use of **guardrail systems, safety net systems, personal fall arrest systems, positioning device systems, or fall restraint systems.** For decking work, once there is no longer a leading edge or at heights greater than 30 feet or 2 stories whichever is less, the CDZ provisions no longer apply.

Employers are encouraged to contact the MIOSHA Construction Safety and Health Division at 517-284-7680 if they have questions regarding jobsite health and safety or compliance issues. The MIOSHA Consultation Education and Training (CET) Division provides training and onsite audit services for residential and commercial builders at the employer’s request, free of charge. The CET Division can be contacted directly at [www.michigan.gov/cetrca](http://www.michigan.gov/cetrca), or at 517-284-7720.